**ARROW BOARD LED INSTALLATION**

1. UNSCREW HALF WAY THE M4 X12 SCREW LOCATED AROUND THE SHROUDS
2. TURN CLOCKWISE TO REMORE SHROUND
3. REMOVE THE SEAL AND FLAX BEHAID THE LED TO REMOVE OLD ONE
4. PLACE NEW LED AND CONNECT WIRES:
	1. BLACK WIRE = NEGATIVE
	2. COLOUR = POSITIVE
5. SCREW SHROUNDS BACK